Universal Robots - UR10e

Payload: 10 kg

Reach: 1300mm = 1,3m

DOF: 6 rotating joints

Working range +-360° for alle led.

Max speed: Base&Shoulder=120°/s – resten=180°/s

Typical TCP speed : 1m/s

Typical power consumption: 350W

Noise level: Less than 65dB(A)

**Communication**

Control frequency: 500Hz

Communication Interfaces: EthernetIP, ProfiNet, USB 2.0 and 3.0

UI: Polyscope graphical user interface on 12 inch touchscreen with mounting

**Sensors**



